**Avalon-Stream VVC** –Quick Reference

**VVC**

For general information see UVVM VVC Framework Essential Mechanisms located in uvvm\_vvc\_framework/doc.

Avalon-Stream Master (see page 2 for Avalon-Stream Slave)

*avalon\_st\_vvc.vhd*

|  |
| --- |
| avalon\_st\_transmit (VVCT, vvc\_instance\_idx, [channel\_value], data\_array, msg, [scope]) |
| Example: avalon\_st\_transmit(AVALON\_ST\_VVCT, 0, v\_channel, v\_data\_array(0 to v\_numWords-1), “Send v\_numWords on v\_channel to DUT”, C\_SCOPE);  Example: avalon\_st\_transmit(AVALON\_ST\_VVCT, 0, (x”01”, x”02”, x”03”, x”04”), “Send 4 bytes to DUT”);  *Note that this procedure can only be called when the AVALON\_ST VVC is instantiated in master mode, i.e. setting the generic constant ‘GC\_MASTER\_MODE’ to true.* |



**Avalon-Stream VVC** –Quick Reference   
Avalon-Stream Slave (see page 1 for Avalon-Stream Master)

|  |
| --- |
| avalon\_st\_receive (VVCT, vvc\_instance\_idx, data\_array\_len, data\_word\_size, msg, [scope]) |
| Example: avalon\_st\_receive(AVALON\_ST\_VVCT, 1, v\_data\_array’length, v\_data\_array(0)’length, “Receive data which is stored in VVC and will be fetched later using fetch\_result() “);  *Note that this procedure can only be called when the AVALON\_ST VVC is instantiated in slave mode, i.e. setting the generic constant ‘GC\_MASTER\_MODE’ to false.* |

|  |
| --- |
| avalon\_st\_expect (VVCT, vvc\_instance\_idx, [channel\_exp], data\_exp, msg, [scope, [alert\_level]]) |
| Example: avalon\_st\_expect(AVALON\_ST\_VVCT, 1, v\_channel, v\_data\_array(0 to v\_numWords-1), “Expect v\_numWords on v\_channel”, C\_SCOPE, ERROR);  Example: avalon\_st\_expect(AVALON\_ST\_VVCT, 1, (x”01”, x”02”, x”03”, x”04”), “Expect 4 bytes”);  *Note that this procedure can only be called when the AVALON\_ST VVC is instantiated in slave mode, i.e. setting the generic constant ‘GC\_MASTER\_MODE’ to false.* |

****

*avalon\_st\_vvc.vhd*

**VVC**

|  |  |
| --- | --- |
| Avalon-Stream VVC Configuration record **´vvc\_config´ --** accessible via **shared\_avalon\_st\_vvc\_config** | **Common VVC procedures applicable for this VVC** |
| |  |  |  | | --- | --- | --- | | **Record element** | **Type** | **C\_AVALON\_ST\_VVC\_CONFIG\_DEFAULT** | | inter\_bfm\_delay | t\_inter\_bfm\_delay | C\_AVALON\_ST\_INTER\_BFM\_DELAY\_DEFAULT | | cmd\_queue\_count\_max | natural | C\_CMD\_QUEUE\_COUNT\_MAX | | cmd\_queue\_count\_threshold | natural | C\_CMD\_QUEUE\_COUNT\_THRESHOLD | | cmd\_queue\_count\_threshold\_severity | t\_alert\_level | C\_CMD\_QUEUE\_COUNT\_THRESHOLD\_SEVERITY | | result\_queue\_count\_max | natural | C\_RESULT\_QUEUE\_COUNT\_MAX | | result\_queue\_count\_threshold | natural | C\_RESULT\_QUEUE\_COUNT\_THRESHOLD | | result\_queue\_count\_threshold\_severity | t\_alert\_level | C\_RESULT\_QUEUE\_COUNT\_THRESHOLD\_SEVERITY | | bfm\_config | t\_avalon\_st\_bfm\_config | C\_AVALON\_ST\_BFM\_CONFIG\_DEFAULT | | msg\_id\_panel | t\_msg\_id\_panel | C\_VVC\_MSG\_ID\_PANEL\_DEFAULT | |  |  |  | | - See UVVM Methods QuickRef for details. |
| **await\_[any]completion**() **enable\_log\_msg**() **disable\_log\_msg**()  **fetch\_result**()  **flush\_command\_queue**() **terminate\_current\_command**() **terminate\_all\_commands**() **insert\_delay**()  **get\_last\_received\_cmd\_idx()** |
| Avalon-Stream VVC Status record signal **´vvc\_status´ --** accessible via **shared\_avalon\_st\_vvc\_status** |
| |  |  |  | | --- | --- | --- | | **Record element** | **Type** |  | | current\_cmd\_idx | natural |  | | | previous\_cmd\_idx | natural |  | | pending\_cmd\_cnt | natural |  | |

VVC target parameters

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Example(s)** | **Description** |
| VVCT | t\_vvc\_target\_record | AVALON\_ST\_VVCT | VVC target type compiled into each VVC in order to differentiate between VVCs. |
| vvc\_instance\_idx | integer | 0 | Instance number of the VVC |

VVC functional parameters

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Example(s)** | **Description** |
| channel\_value  channel\_exp | std\_logic\_vector | x”01” | Channel number for the data being transferred or expected.  The value is limited by max\_channel in the bfm\_config. |
| data\_array  data\_exp | t\_slv\_array | (x“D0D1”, x“D2D3”) | An array of SLVs containing the data to be sent/received.  data\_array(0) is sent/received first, while data\_array(data\_array’high) is sent/received last.  For clarity, data\_array is required to be ascending, for example defined by the test sequencer as follows:  variable v\_data\_array : t\_slv\_array(0 to C\_MAX\_WORDS-1)(C\_MAX\_WORD\_LENGTH-1 downto 0);  For simplicity, the word\_length can only be the size of the configured symbol or the size of the data bus.  variable v\_data\_array : t\_slv\_array(0 to C\_MAX\_WORDS-1)(C\_SYMBOL\_WIDTH-1 downto 0);  variable v\_data\_array : t\_slv\_array(0 to C\_MAX\_WORDS-1)(C\_DATA\_BUS\_LENGTH-1 downto 0); |
| data\_array\_len | natural | 20 | Length of the data\_array expected to be received (number of words). |
| data\_word\_size | natural | 8 | Size of the data words in the data\_array expected to be received. |
| alert\_level | t\_alert\_level | ERROR or TB\_WARNING | Set the severity for the alert that may be asserted by the procedure. |
| msg | string | “Send data” | A custom message to be appended in the log/alert |
| scope | string | “AVALON\_ST\_VVC” | A string describing the scope from which the log/alert originates.  In a simple single sequencer typically "AVALON\_ST\_BFM". In a verification component typically "AVALON\_ST\_VVC ". |

VVC entity signals

|  |  |  |
| --- | --- | --- |
| **Name** | **Type** | **Description** |
| clk | std\_logic | VVC Clock signal |
| avalon\_st\_vvc\_if | t\_avalon\_st\_if | See Avalon-Stream BFM documentation |

VVC entity generic constants

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Default** | **Description** |
| GC\_VVC\_IS\_MASTER | boolean | - | Set to true when this VVC instance is an Avalon-Stream master (data is output from BFM).  Set to false when this VVC is an Avalon-Stream slave (data is input to BFM.) |
| GC\_CHANNEL\_WIDTH | integer | 1 | Width of the Avalon-Stream channel signal.  *Note 1*: if CHANNEL is wider than 8, increase the value of the constant C\_VVC\_CMD\_CHAN\_MAX\_LENGTH in transaction\_pkg.  *Note 2*: If the CHANNEL signal is not used, refer to description in Section 5. |
| GC\_DATA\_WIDTH | integer | - | Width of the Avalon-Stream data bus.  *Note*: if DATA is wider than 512, increase the value of the constant C\_VVC\_CMD\_WORD\_MAX\_LENGTH in transaction\_pkg. |
| GC\_DATA\_ERROR\_WIDTH | integer | 1 | Width of the Avalon-Stream data error signal.  *Note*: If the DATA\_ERROR signal is not used, refer to description in Section 5. |
| GC\_EMPTY\_WIDTH | integer | 1 | Width of the Avalon-Stream empty signal.  *Note*: If the EMPTY signal is not used, refer to description in Section 5. |
| GC\_INSTANCE\_IDX | natural | - | Instance number to assign the VVC. |
| GC\_AVALON\_ST\_BFM\_CONFIG | t\_avalon\_st\_bfm\_config | C\_AVALON\_ST\_BFM\_  CONFIG\_DEFAULT | Configuration for the Avalon-Stream BFM, see Avalon-Stream BFM documentation. |
| GC\_CMD\_QUEUE\_COUNT\_MAX | natural | 1000 | Absolute maximum number of commands in the VVC command queue. |
| GC\_CMD\_QUEUE\_COUNT\_THRESHOLD | natural | 950 | An alert will be generated when reaching this threshold to indicate that the command queue is almost full. The queue will still accept new commands until it reaches C\_CMD\_QUEUE\_COUNT\_MAX. |
| GC\_CMD\_QUEUE\_COUNT\_THRESHOLD\_SEVERITY | t\_alert\_level | WARNING | Alert severity which will be used when command queue reaches GC\_CMD\_QUEUE\_COUNT\_THRESHOLD. |
| GC\_RESULT\_QUEUE\_COUNT\_MAX | natural | 1000 | Maximum number of unfetched results before result\_queue is full. |
| GC\_RESULT\_QUEUE\_COUNT\_THRESHOLD | natural | 950 | An alert with severity ‘result\_queue\_count\_threshold\_severity’ will be issued if result queue exceeds this count. Used for early warning if result queue is almost full. Will be ignored if set to 0. |
| GC\_RESULT\_QUEUE\_COUNT\_THRESHOLD\_SEVERITY | t\_alert\_level | WARNING | Severity of alert to be initiated if exceeding result\_queue\_count\_threshold. |

VVC details

All VVC procedures are defined in vvc\_methods\_pkg (dedicated this VVC), and uvvm\_vvc\_framework.td\_vvc\_framework\_common\_methods\_pkg (common VVC procedures).   
It is also possible to send a multicast to all instances of a VVC with ALL\_INSTANCES as parameter for vvc\_instance\_idx.   
*Note: Every procedure here can be called without the optional parameters enclosed in [ ].*

# VVC procedure details

|  |  |
| --- | --- |
| **Procedure** | **Description** |
| **avalon\_st\_transmit()** | **avalon\_st\_transmit (VVCT, vvc\_instance\_idx, channel\_value, data\_array, msg, [scope])**  The avalon\_st\_transmit() VVC procedure adds a transmit command to the Avalon-Stream VVC executor queue, which will run as soon as all preceding commands have completed. When the command is scheduled to run, the executor calls the Avalon-Stream BFM avalon\_st\_transmit() procedure, described in the Avalon-Stream BFM QuickRef.  The avalon\_transmit() procedure can only be called when the AVALON VVC is instantiated in master mode, i.e. setting the generic constant ‘GC\_MASTER\_MODE’ to true. |
| **avalon\_st\_receive()** | **avalon\_st\_receive (VVCT, vvc\_instance\_idx, data\_array\_len, data\_word\_size, msg, [scope])**  The avalon\_st\_receive() VVC procedure adds a receive command to the Avalon-Stream VVC executor queue, which will run as soon as all preceding commands have completed. When the command is scheduled to run, the executor calls the Avalon-Stream BFM avalon\_st\_receive() procedure, described in the Avalon-Stream BFM QuickRef.  The avalon\_receive() procedure can only be called when the AVALON VVC is instantiated in slave mode, i.e. setting the generic constant ‘GC\_MASTER\_MODE’ to false.  The value received from the DUT will not be returned in this procedure call since it is non-blocking for the sequencer/caller, but the received data and metadata will be stored in the VVC for a potential future fetch (see example with *fetch\_result* below).  **Example with fetch\_result() call**: Result is placed in **v\_result**  variable v\_cmd\_idx : natural; -- Command index for the last receive  variable v\_result : work.vvc\_cmd\_pkg.t\_vvc\_result; -- Result from receive (data and metadata)  (…)  avalon\_st\_receive(AVALON\_ST\_VVCT, 1, v\_data\_array’length, v\_data\_array(0)’length, “Receive data in VVC”);  v\_cmd\_idx := get\_last\_received\_cmd\_idx(AVALON\_ST\_VVCT, 1);  await\_completion(AVALON\_ST\_VVCT, 1, 1 ms, “Wait for receive to finish”);  fetch\_result(AVALON\_ST\_VVCT, 1, v\_cmd\_idx, **v\_result**, “Fetching result from receive operation”); |
| **avalon\_st\_expect()** | **avalon\_st\_expect (VVCT, vvc\_instance\_idx, channel\_exp, data\_exp, msg, [scope, [alert\_level]])**  The avalon\_st\_expect() VVC procedure adds an expect command to the Avalon-Stream VVC executor queue, which will run as soon as all preceding commands have completed. When the command is scheduled to run, the executor calls the Avalon-Stream BFM avalon\_st\_expect() procedure, described in the Avalon-Stream BFM QuickRef.  The avalon\_expect() procedure can only be called when the AVALON VVC is instantiated in slave mode, i.e. setting the generic constant ‘GC\_MASTER\_MODE’ to false. |
|  |  |

# VVC Configuration

|  |  |  |  |
| --- | --- | --- | --- |
| **Record element** | **Type** | **C\_AVALON\_ST\_VVC\_CONFIG\_DEFAULT** | **Description** |
| inter\_bfm\_delay | t\_inter\_bfm\_delay | C\_AVALON\_ST\_INTER\_BFM\_DELAY\_DEFAULT | Delay between any requested BFM accesses towards the DUT. - TIME\_START2START: Time from a BFM start to the next BFM start   (A TB\_WARNING will be issued if access   takes longer than TIME\_START2START).  - TIME\_FINISH2START: Time from a BFM end to the next BFM start. Any insert\_delay() command will add to the above minimum delays, giving for instance the ability to skew the BFM starting time. |
| cmd\_queue\_count\_max | natural | C\_CMD\_QUEUE\_COUNT\_MAX | Maximum pending number in command queue before queue is full. Adding additional commands will result in an ERROR. |
| cmd\_queue\_count\_threshold | natural | C\_CMD\_QUEUE\_COUNT\_THRESHOLD | An alert with severity “cmd\_queue\_count\_threshold\_severity” will be issued if command queue exceeds this count. Used for early warning if command queue is almost full. Will be ignored if set to 0. |
| cmd\_queue\_count\_threshold\_severity | t\_alert\_level | C\_CMD\_QUEUE\_COUNT\_THRESHOLD\_SEVERITY | Severity of alert to be initiated if exceeding cmd\_queue\_count\_threshold |
| result\_queue\_count\_max | natural | C\_RESULT\_QUEUE\_COUNT\_MAX | Maximum number of unfetched results before result\_queue is full. |
| result \_queue\_count\_threshold | natural | C\_RESULT\_QUEUE\_COUNT\_THRESHOLD | An alert with severity ‘result\_queue\_count\_threshold\_severity’ will be issued if result queue exceeds this count. Used for early warning if result queue is almost full. Will be ignored if set to 0. |
| result \_queue\_count\_threshold\_severity | t\_alert\_level | C\_ RESULT\_QUEUE\_COUNT\_THRESHOLD\_SEVERITY | Severity of alert to be initiated if exceeding result\_queue\_count\_threshold. |
| bfm\_config | t\_avalon\_st\_bfm\_config | C\_AVALON\_ST\_BFM\_CONFIG\_DEFAULT | Configuration for Avalon-Stream BFM. See quick reference for Avalon-Stream BFM. |
| msg\_id\_panel | t\_msg\_id\_panel | C\_VVC\_MSG\_ID\_PANEL\_DEFAULT | VVC dedicated message ID panel. |

The configuration record can be accessed from the Central Testbench Sequencer through the shared variable array, e.g.:

shared\_avalon\_st\_vvc\_config(1).inter\_bfm\_delay.delay\_in\_time := 50 ns;

shared\_avalon\_st\_vvc\_config(1).bfm\_config.clock\_period := 10 ns;

# VVC Status

The current status of the VVC can be retrieved during simulation. This is achieved by reading from the shared variable shared\_avalon\_st\_vvc\_status record from the test sequencer. The record contents can be seen below:

|  |  |  |
| --- | --- | --- |
| **Record element** | **Type** | **Description** |
| current\_cmd\_idx | natural | Command index currently running |
| previous\_cmd\_idx | natural | Previous command index to run |
| pending\_cmd\_cnt | natural | Pending number of commands in the command queue |

# Activity watchdog

The VVCs support an activity watchdog which monitors VVC activity and will alert if no VVC activity is registered within a selected timeout value. The VVCs will register their presence to the activity watchdog at start-up, and report when busy and not, using dedicated activity watchdog methods and triggering the global\_trigger\_activity\_watchdog signal, during simulations.

Include activity\_watchdog(num\_exp\_vvc, timeout, alert\_level, msg) in the testbench to start using the activity watchdog.   
More information can be found in UVVM Essential Mechanisms PDF in the UVVM VVC Framework doc folder.

# VVC Interface

In this VVC, the interface has been encapsulated in a signal record of type *t\_avalon\_st\_if* in order to improve readability of the code. Since the Avalon-Stream interface buses can be of arbitrary size, the interface std\_logic\_vectors have been left unconstrained. These unconstrained SLVs needs to be constrained when the interface signals are instantiated. For this interface, this could look like:

signal avalon\_st\_if : t\_avalon\_st\_if (

channel(C\_CHANNEL\_WIDTH-1 downto 0),

data(C\_DATA\_WIDTH-1 downto 0),

data\_error(C\_ERROR\_WIDTH-1 downto 0),

empty(log2(C\_DATA\_WIDTH/C\_SYMBOL\_WIDTH)-1 downto 0));

The widths of *channel, data\_error* and *empty* are declared even when not used or connected to DUT.

Set the widths of unused signals to 1, for example C\_CHANNEL\_WIDTH = 1.

# Additional Documentation

Additional documentation about UVVM and its features can be found under “/uvvm\_vvc\_framework/doc/”.

For additional documentation on the Avalon-Stream standard, refer to “Avalon® Interface Specifications, Chapter: Avalon Streaming Interfaces”, document number MNL-AVABUSREF, available from Intel.

# Compilation

Avalon-Stream VVC must be compiled with VHDL 2008.   
It is dependent on the following libraries

* ***UVVM Utility Library (UVVM-Util), version 2.10.0 and up***
* ***UVVM VVC Framework, version 2.7.0 and up***
* ***Avalon-Stream BFM***
* ***Bitvis VIP Scoreboard***

Before compiling the Avalon-Stream VVC, assure that uvvm\_vvc\_framework, uvvm\_util and bitvis\_vip\_scoreboard have been compiled.

See UVVM Essential Mechanisms located in uvvm\_vvc\_framework/doc for information about compile scripts.

**Compile order for the Avalon-Stream VVC:**

|  |  |  |
| --- | --- | --- |
| **Compile to library** | **File** | **Comment** |
| bitvis\_vip\_avalon\_st | avalon\_st\_bfm\_pkg.vhd | Avalon-Stream BFM |
| bitvis\_vip\_avalon\_st | transaction\_pkg.vhd | Avalon-Stream transaction package with DTT types, constants etc. |
| bitvis\_vip\_avalon\_st | vvc\_cmd\_pkg.vhd | Avalon-Stream VVC command types and operations |
| bitvis\_vip\_avalon\_st | ../uvvm\_vvc\_framework/src\_target\_dependent/td\_target\_support\_pkg.vhd | UVVM VVC target support package, compiled into the Avalon-Stream VVC library. |
| bitvis\_vip\_avalon\_st | ../uvvm\_vvc\_framework/src\_target\_dependent/td\_vvc\_framework\_common\_methods\_pkg.vhd | UVVM framework common methods compiled into the Avalon-Stream VVC library |
| bitvis\_vip\_avalon\_st | vvc\_methods\_pkg.vhd | Avalon-Stream VVC methods |
| bitvis\_vip\_avalon\_st | ../uvvm\_vvc\_framework/src\_target\_dependent/td\_queue\_pkg.vhd | UVVM queue package for the VVC |
| bitvis\_vip\_avalon\_st | ../uvvm\_vvc\_framework/src\_target\_dependent/td\_vvc\_entity\_support\_pkg.vhd | UVVM VVC entity support compiled into the Avalon-Stream VVC library |
| bitvis\_vip\_avalon\_st | avalon\_st\_vvc.vhd | Avalon-Stream VVC |

# Simulator compatibility and setup

See README.md for a list of supported simulators.

For required simulator setup see ***UVVM-Util*** Quick reference.

IMPORTANT

This is a simplified Verification IP (VIP) for Avalon-Stream. The given VIP complies with the basic Avalon-Stream protocol and thus allows a normal access towards an Avalon-Stream interface. This VIP is not Avalon-Stream protocol checker. For a more advanced VIP please contact Bitvis AS at [support@bitvis.no](mailto:support@bitvis.no)

Disclaimer: This IP and any part thereof are provided "as is", without warranty of any kind, express or implied, including but not limited to the warranties of merchantability, fitness for a particular purpose and noninfringement.  
In no event shall the authors or copyright holders be liable for any claim, damages or other liability, whether in an action of contract, tort or otherwise, arising from, out of or in connection with this IP.

**INTELLECTUAL**

**PROPERTY**